interface fastEthernet 0/1

switchport mode trunk

switchport trunk allowed vlan 10,20,30

exit

interface fastEthernet 0/2

switchport mode trunk

switchport trunk allowed vlan 10,20,30

exit

interface fastEthernet 0/3

switchport mode trunk

switchport trunk allowed vlan 10,20,30

exit

interface fastEthernet 0/4

switchport mode trunk

switchport trunk allowed vlan 10,20,30

exit

interface fastEthernet 0/5

switchport mode trunk

switchport trunk allowed vlan 10,20,30

exit